K56 7x7 24pkt Card Stand Assembly Instructions
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What’s in the box:


A. 4x Pocket Panel
B. 1x Top Core
C. 1x Middle Core
D. 1x Bottom Core
E. 12x Bolt
F.  12x Washer
G. 12x Wingnut
H. 1x Pole
I.  1x Base (see 5 Way Base Assembly Instructions)
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Find a flat surface and lay down a Pocket Panel, then hold the Bottom Core against the holes in the plate at the bottom end of the Panel and insert the Bolts up through the Panel, put the Washer and Wingnut over the Bolt and loosely hand tighten, repeat with the Middle core and the Top Core.
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	Roll the unit then place the next Pocket Panel on top of the Cores. Insert all three Bolts through the plates on the Pocket Panel and through the Cores, add the Washers then the Wingnuts from underneath and loosely tighten all by hand one by one.
Roll the stand so Pocket Panels can be attached on top. Repeat until all Pocket Panels are fixed to the stand.
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	Pick the unit up and stand it upright.
Looking at the stand from above you’ll need to slide the Pocket Panels sideways to ensure equal spacing, on the example to the left the red highlight shows where the pockets need to sit - up against the back of the next, repeat this clockwise four times until it looks like the example. When you’re happy with the alignment tighten down all Wingnuts.
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 Take the Pole and slot it over the Threaded spigot.
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Tip the stand and the Pole onto their sides.

Push the Pole through the centre of the Bottom core until it hits the centre of the Middle core.

When in place the unit can be stood upright.

	[image: ]
	






Your stand is complete, you can now load it with products, make sure to load evenly on opposite sides to avoid imbalances when turning.
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