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4 Crate Display Unit with Wheels (CRATE/1)
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12 loining Bolts
2xAllen Keys

Step 1.
Place the base crate (with wheels) an
the floor on it’s side so you can access
the drill holes on the tap.

Thread thejoining bolts =
thraugh Crate 2 and
into the top of Crate 1.
Tighten with allen keys
provided and then
stand the crates upright
(as shown >>)
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Step 2.
Place Crate 3 on top of
Crate 2 ensuringthe drill
holes line up. Thread the
joiningbalts through
Crate 3 into Crate 2 and
tighten with allen keys
provided

Step 3.
Place Crate 4 on top of
Crate 3 ensuringthe dril 7
holes line up. Thread the
joining balts through
Crate 4 into Crate 3 and
tighten with allen keys
provided

Step 4.
Yaur crate display is
ready! Release the

braked whesls to move -y
into position and place |
yaur products
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