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PARTS SUPPLIED:
3xPremium Crates

1 xBase Crate [with Wheels if
selectec]

9 loining Bolts

2x Allen Keys

Step 1.
Place the base crate (with wheels) an
the floor on it’s side so you can access
the drill holes on the tap.

Thread thejoining bolts = .
through Crate 2 and |

into the top of Crate 1. ‘\‘ @
Tighten with allen keys

provided and then !

stand the crates upright
(as shown >>)
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4 Crate Display Unit (CRATE/1)
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Step 2.

Place Crate 3 on top of
Crate 2 ensuringthe drill
holes line up. Thread the
joiningbalts through
Crate 3 into Crate 2 and
tighten with allen keys
provided
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Step 3.

Place Crate 4 on top of
Crate 3 ensuringthe drill
holes line up. Thread the
joining balts through
Crate 4 into Crate 3 and
tighten with allen keys
provided

Step 4.
Your crate display is

ready! Release the

braked wheals to move
into position and place |
your products, |
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